A red and white sign

Description automatically generated with low confidence

User Guide:

Azure IoT Hub Device Update for the SAM E54 Xplained Pro Development Board

Table of Contents

[Overview 3](#_Toc134270199)

[Prepare Azure Resources 6](#_Toc134270200)

[Create an IoT Hub 6](#_Toc134270201)

[Register a Device with the IoT Hub 8](#_Toc134270202)

[Create Device Update Account and Instance 9](#_Toc134270203)

[Prepare the New Firmware 10](#_Toc134270204)

[Clone/Download the Example Project 10](#_Toc134270205)

[Build New Firmware Image 10](#_Toc134270206)

[Prepare New Firmware for the Simulated Leaf Device 12](#_Toc134270207)

[Generate Import Manifest 12](#_Toc134270208)

[Upload Firmware and Manifest 13](#_Toc134270209)

[Prepare the Device 15](#_Toc134270210)

[Revert to the Previous Firmware Version 16](#_Toc134270211)

[Program and Run the Device 16](#_Toc134270212)

[Deploy New Firmware 18](#_Toc134270213)

[Add a Tag to Your Device 18](#_Toc134270214)

[Deploy New Firmware Update 18](#_Toc134270215)

[Clean Up Resources 24](#_Toc134270216)

[Next Steps 25](#_Toc134270217)

# Overview

The following steps detail how to configure, build and execute the [Device Update for IoT Hub](https://docs.microsoft.com/azure/iot-hub-device-update/) example on the Microchip SAM E54 Xplained Pro. For this example, we will learn how to:

* Create Azure IoT Hub and Device Update for IoT Hub resources.
* Prepare the firmware for the dev board and the manifest file required for it.
* Prepare the firmware for the simulated leaf device for [proxy update](https://docs.microsoft.com/azure/iot-hub-device-update/device-update-proxy-updates) and manifest file required for it.
* Upload the files and create the group for the device in the Device Update for IoT Hub.
* Deploy the firmware to the device and observe the result of it.

The tool uses in the sample is MPLAB X IDE 6.05: <https://www.microchip.com/mplab/mplab-x-ide>.

You will also need MPLAB XC32/32++ Compiler 4.1.0 or later to build the example projects: <https://www.microchip.com/mplab/compilers>

A circuit board

Description automatically generated

Figure Microchip SAM E54 Xplained Pro

The sample distribution zip file contains the following sub-folders:

|  |  |
| --- | --- |
| Folder | Contents |
| *common\_hardware\_code* | Common code for SAM E54 board |
| *docs* | User guides |
| *netxduo* | NetX Duo source code |
| *sample\_azure\_iot\_embedded\_sdk\_pnp* | Sample project to connect to Azure IoT Hub using Azure IoT Middleware for Azure RTOS |
| *same54\_lib* | SAM E54 drivers |
| *threadx* | ThreadX source code |
| *filex* | FileX source code |

# Prepare Azure Resources

## Create an IoT Hub

You can use the [Azure Command Line Interface (CLI)](https://learn.microsoft.com/en-us/cli/azure/install-azure-cli) to create an IoT hub that handles events and messaging for your device.

1. Log into your Azure [portal](https://portal.azure.com/) account and click on the **Cloud Shell** icon located at the top of the web page (you may be prompted to create a storage account in order to use Cloud Shell)

CLICK

Graphical user interface, text, application, chat or text message

Description automatically generated

1. In the upper left-hand corner of the **Cloud Shell** pane, confirm that ***PowerShell*** is selected

CLICK

Graphical user interface

Description automatically generated with low confidence

1. At the PS prompt, run the [az extension add](https://docs.microsoft.com/cli/azure/extension?view=azure-cli-latest#az-extension-add) command to add the Microsoft Azure IoT Extension for Azure CLI to your CLI shell. The IoT Extension adds IoT Hub, IoT Edge, and IoT Device Provisioning Service (DPS) specific commands to the Azure CLI.

az extension add --name azure-iot

1. Run the [az account list](https://learn.microsoft.com/en-us/cli/azure/account?view=azure-cli-latest#az-account-list) command to see the list of subscriptions accessible by your Azure account

az account list

1. Run the [az account set](https://learn.microsoft.com/en-us/cli/azure/account?view=azure-cli-latest#az-account-set) command to select the specific subscription you want to use for creating the Azure resources

az account set --subscription "{MySubscriptionName}"

1. Run the 1 (or 2) command(s) required to create a resource group. For example, if your company’s policy requires specific tags be added to a resource group, you can create a “tags” variable to point to a list of all the tag name/value pairs required before creating the resource group. Otherwise if no tags are needed, just run the **New-AzResourceGroup** command and without the -tag option. To set a specific location for your resource group, run [az account list-locations](https://docs.microsoft.com/cli/azure/account?view=azure-cli-latest#az-account-list-locations) to see a list of all available regions.

$tags=@{"name1"="val1";"name2"="val2";"name3"="val3”;etc}

New-AzResourceGroup -Name {MyResourceGroup} -Location {MyLocation} [-tag $tags]

For example, the following 2 command lines will create a resource group named ***ADU\_TestGroup*** with a location of ***westus*** along with 8 different tags which might be used for a company’s policy for accounting purposes:

$tags=@{"BusinessOwner"="Rob Stein - C07707"; "CostCenter"="SESE00"; "CreatedBy"="Randy Wu - C14166"; "CreationDate"="20230421"; "Env"="DEV"; "Group"="N/A"; "ManagedBy"="Randy Wu - C14166"; "SNOWTicket"="N/A"}

New-AzResourceGroup -Name ADU\_TestGroup -Location westus -tag $tags

NOTE: If using Bash (UNIX) CLI, execute the following command line:

az group create --name {MyResourceGroup} --location {MyLocation} [--tags name1="value1" name2="value2" name3="value3" etc...]

…for example:

az group create --name ADU\_TestGroup --location westus --tags BusinessOwner="Rob\_Stein - C07707" CostCenter=SESE00 CreatedBy="Randy Wu - C14166" CreationDate=20230421 Env=DEV Group=N/A ManagedBy="Randy Wu - C14166 SNOWTicket=N/A

1. Run the [az iot hub create](https://docs.microsoft.com/cli/azure/iot/hub?view=azure-cli-latest#az-iot-hub-create) command to create an IoT hub. It might take a few minutes for Azure to finalize the creation of the IoT hub…

Replace YourIotHubName below with the name you choose for your IoT Hub. An IoT Hub name must be globally unique in Azure.

az iot hub create --resource-group {MyResourceGroup} --name {YourIoTHubName}

… for example:

az iot hub create –resource-group "ADU-TestGroup" --name "ADU-IoTHub"

1. After the IoT hub is created, view the JSON output in the console, and copy the hostName value to a safe place. You will use this value in a later step. The hostName value will be in the following format:

{YourIoTHubName}.azure-devices.net

**[TIP]** You can look up the host name again by using the following command to list all the IoT Hub host names that are tied to your portal account:

az iot hub list --query "[].{hostname:properties.hostName}" --output table

## Register a Device with the IoT Hub

In this section, you create a new device instance and register it with the IoT Hub you created. You will use the connection information for the newly registered device to securely connect your physical device in a later section.

1. In your console, run the [az iot hub device-identity create](https://docs.microsoft.com/cli/azure/ext/azure-cli-iot-ext/iot/hub/device-identity?view=azure-cli-latest#ext-azure-cli-iot-ext-az-iot-hub-device-identity-create) command. This creates the simulated device identity.

YourIotHubName. Replace this placeholder below with the name you chose for your IoT hub.

MyDevKit. You can use this name directly for the device in CLI commands in this tutorial. Choose a meaningful name for your kit (e.g. ***WFI32-IoT***)

az iot hub device-identity create --device-id "{MyDevKit}" --hub-name "{YourIoTHubName}"

… for example:

az iot hub device-identity create --device-id "WFI32-IoT" --hub-name "ADU-IoTHub"

1. After the device is created, view the JSON output in the console, copy and save the deviceId and primaryKey values to use in a future step.

Confirm that you have the copied and saved the following values from the JSON output to use in the next section:

* hostName
* deviceId
* primaryKey

TIP: You can get the primaryKey at any time by executing the following command in the Azure CLI:

az iot hub device-identity show --hub-name {YourIoTHubName} --device-id {MyDevKit}

… for example:

az iot hub device-identity show --hub-name "ADU-IoTHub" --device-id "WFI32-IoT"

## Create Device Update Account and Instance

Click on one of the following hyperlinks to create a Device Update account and instance using one of the following methods:

* Azure [portal](https://learn.microsoft.com/en-us/azure/iot-hub-device-update/create-device-update-account?tabs=portal)
* Azure [CLI](https://learn.microsoft.com/en-us/azure/iot-hub-device-update/create-device-update-account?tabs=cli)

# Prepare the New Firmware

To connect the device to Azure, you'll modify a configuration file for Azure IoT settings, build and flash the image to the device.

## Clone/Download the Example Project

Using the Git [command line](https://git-scm.com/book/en/v2/Getting-Started-The-Command-Line) or [Desktop](https://desktop.github.com/) tool, clone the repository located at the URL specified in the following command line:

git clone https://github.com/MicrochipTech/AzureDemo\_DeviceUpdate

As an alternative, you can simply go to the specified URL and download a ZIP file of the repository:

Graphical user interface, text, application, email

Description automatically generated

2

1

## Build New Firmware Image

1. Launch the MPLAB X IDE and select ***File > Open Project*** and select the following projects from the extracted zip file:
   * threadx
   * netxduo
   * same54\_lib
   * sample\_azure\_iot\_embedded\_sdk\_pnp
2. Select the sample\_azure\_iot\_embedded\_sdk\_pnp sample, right click on it on in the left ***Projects*** pane and select ***Set as main project***.
3. Expand the Header files folder to open sample\_config.h to set the Azure IoT device information constants to the values that you saved after you created Azure resources.

|  |  |
| --- | --- |
| Constant name | Value |
| HOST\_NAME | {Your IoT hub hostName value} |
| DEVICE\_ID | {Your deviceID value} |
| DEVICE\_SYMMETRIC\_KEY | {Your primaryKey value} |

1. In the same folder, open ***sample\_azure\_iot\_embedded\_sdk\_adu.c,*** modify the firmware version to mimic it is a new firmware that will be deployed from Device Update.

#define SAMPLE\_DEVICE\_INSTALLED\_CRITERIA "2.0.0"

#define SAMPLE\_LEAF\_DEVICE\_INSTALLED\_CRITERIA "2.0.0"

1. Make sure all of the sample project’s dependent libraries (threadx, netxduo, same54\_lib) are built by right-clicking on each project in the ***Projects*** pane and selecting ***Clean and Build***.
2. MPLAB X [does not create .bin file by default](https://microchipsupport.force.com/s/article/MPLAB-X-IDE---Generating-binary-file---xc32-Compiler#:~:text=Answer.%20MPLAB%20X%20does%20not%20create%20.bin%20file,build%20%E2%80%99%20option%20and%20insert%20the%20following%20command.). Right click on the **sample\_azure\_iot\_embedded\_sdk\_pnp** project, select **Properties** > **Building**, check the box “Execute this line after build”, and insert the following command into the text box:

${MP\_CC\_DIR}/xc32-objcopy -I ihex -O binary "${DISTDIR}/${PROJECTNAME}.${IMAGE\_TYPE}.hex" "${DISTDIR}/${PROJECTNAME}.${IMAGE\_TYPE}.bin"

Graphical user interface, text, application, email

Description automatically generated

1. The binary firmware will be generated in ***mplab\sample\_azure\_iot\_embedded\_sdk\_pnp\*** ***dist\default\production.*** Copy the ***\*.bin*** file to ***mplab\tools\AzureDeviceUpdateScripts*** folder where the scripts for generating manifest files are within. It is optional but recommended also change the file name that matches with your firmware version such as ***firmware\_2.0.0.bin****.*

Now you have prepared the new firmware for the dev board that will be uploaded to Device Update for IoT Hub.

## Prepare New Firmware for the Simulated Leaf Device

Even though we do not physically connect any leaf devices to the dev board we are using, it is a common scenario for your MCU device that you might have one or more leaf devices connect to it via UART or USB as peripherals or sensors. For this example, we just use a simulated leaf device and push an empty firmware to demonstrate the experience. To do that:

Create a file and name it ***leaf\_firmware\_2.0.0.bin*** and save in the same ***mplab/tools/AzureDeviceUpdateScripts*** folder with this PowerShell command:

New-Item "leaf\_firmware\_2.0.0.bin" -ItemType File -Value "Empty leaf firmware"

A picture containing text, screenshot, font

Description automatically generated

## Generate Import Manifest

An [import manifest](https://docs.microsoft.com/azure/iot-hub-device-update/import-concepts) is a JSON file that defines important information about the update that you are importing that is required by the Device Update for IoT Hub. You can learn the detailed steps about importing new update from [here](https://docs.microsoft.com/azure/iot-hub-device-update/import-update). For this sample:

1. Ensure you have installed [PowerShell v7.0](https://github.com/PowerShell/PowerShell/releases/tag/v7.0.3) or above.
2. In a PowerShell window, navigate to **AzureDemo\_DeviceUpdate > ATSAME54-XPRO > *mplab > tools*** ***> AzureDeviceUpdateScripts*** directory and run:

Set-ExecutionPolicy -ExecutionPolicy Bypass -Scope Process

You may see the following result which is fine and can be ignored:



1. Run the following script and follow the prompt to generate the manifest files for the dev board and the simulated leaf device:

.\CreateSAME54Update.ps1

Supply values for the following parameters:

(Type !? for Help.)

Version: 2.0.0

HostPath: ./firmware\_2.0.0.bin

LeafPath: ./leaf\_firmware\_2.0.0.bin

Replace the values with the actual path and version you have for the firmware. You can also type !? for the help.

1. Upon successful completion of the script, all files required (to upload into the Device Update service) is generated in the folder named ***MICROCHIP.SAME54.2.0.0***

A screenshot of a computer

Description automatically generated with low confidence

## Upload Firmware and Manifest

1. Access your Azure [portal](https://portal.azure.com/) account to find the IoT Hub resource which was created earlier. You may have to first access the resource group that contains it in order to find the IoT Hub. When the IoT Hub has been found in your Azure portal, click on the IoT Hub name to access its configuration details.
2. Using the left-hand navigation pane, select **Device Management > Updates**

Graphical user interface, text, application, chat or text message

Description automatically generated

CLICK

1. Locate the **Updates** tab and then select **Import a new update**

Graphical user interface, text, application

Description automatically generated with medium confidence

CLICK

1. Choose **+ Select from storage container**. If no storage accounts show up in the list, create a new one now by selecting **+ Storage account**.
2. From the list of Storage accounts, click on the name of the newly-created (or pre-existing) storage account that you would like to use for storing the manifest files and binary images required for the Device Update process.
3. You should now be on the ***Containers*** page. If no containers show up in the list, select **+ Container** and enter in a name for the new container. Click on the **Create** button.
4. In the list of existing Containers, click on the name of the container that you would like to use for storing the Device Update files.
5. Select **Upload** and browse to (or drag-and-drop) all of firmware image and manifest files required for the deployment from the **MICROCHIP.SAME54.1.1.0** folder.
6. Click on the **Upload** button. You should see the message “Successfully uploaded blob(s)” and then see a list of all the uploaded files (4 blobs total):

Text

Description automatically generated with medium confidence

A screenshot of a computer

Description automatically generated with medium confidence

A screenshot of a computer program

Description automatically generated with low confidence

Now you have the new firmware images and manifest files uploaded into a container, which prepares you for creating a deployment in a future section. It’s now time to turn our attention to the device and get it up and running to receive the new firmware.

# Prepare the Device

We will build and run the same device application but for a previous version, so that later we can observe the new firmware being deployed to update to the newer version.

## Revert to the Previous Firmware Version

1. In MPLAB, open ***sample\_azure\_iot\_embedded\_sdk\_adu.c***, modify version to an older one to mimic current firmware:


#define SAMPLE\_DEVICE\_INSTALLED\_CRITERIA "1.0.0"

#define SAMPLE\_LEAF\_DEVICE\_INSTALLED\_CRITERIA "1.0.0"

1. Now rebuild the ***sample\_azure\_iot\_embedded\_sdk\_pnp*** project.

## Program and Run the Device

1. Use the Micro USB cable to connect the Debug USB port on the Microchip SAM E54, and then connect it to your computer.
2. Use the Ethernet cable to connect the Microchip SAM E54 to an Ethernet port.
3. Verify the serial port in your OS’s device manager. It should show up as a Virtual COM port:



1. Open your favorite serial terminal program such as [Putty](https://www.chiark.greenend.org.uk/~sgtatham/putty/) or [Tera Term](https://ttssh2.osdn.jp/index.html.en) and connect to the COM port discovered above at ***115200*** baud
2. In MPLAB, navigate to the main toolbar and click the ***Make and Program Device*** icon.

CLICK



1. Go to the terminal program window. As the demo project runs on the device, it continuously prints out status information to the terminal output window. Check the terminal output to verify that there are no error messages and that there is a message stating that the device has “Connected to IoTHub”. Note the output message towards the end that displays the installed criteria version number.

NOTE: The terminal output content may vary depending on which example project you choose to build and run. Keep the terminal window open to monitor device output in subsequent steps.

A screenshot of a computer program

Description automatically generated with medium confidence

# Deploy New Firmware

## Add a Tag to Your Device

1. Confirm that the device application is still running from the previous step (i.e. normal execution was never interrupted).
2. Log into the Azure [portal](https://portal.azure.com/) and navigate to the IoT Hub (you may need to access the resource group that’s tied to the IoT Hub in order to view it).
3. Using the left-hand navigation pane, select ***Device Management > Devices***.
4. Your device ID should show up in the list of devices; click directly on its name in the list.
5. Click on the ***Device Twin*** tab.
6. Create a deployment group by adding a tag to the Device Twin:

"tags": {

"ADUGroup": "{MyDeploymentGroupName}"

}

Graphical user interface, text, application

Description automatically generated

NOTE: To remove any tag in the future, the tag value can be set to ‘null’

1. Click on the ***Save*** icon in the upper left-hand corner of the page, then click on the **X** in the upper right-hand corner of the page to close the ***Device twin*** view.

## Deploy New Firmware Update

1. In the Azure [portal](https://portal.azure.com/), navigate to the IoT Hub that you previously connected to your Device Update instance (you may need to navigate to the resource group which contains the IoT Hub in order to access it).
2. Using the left-hand navigation pane, select ***Devices > Updates***
3. Select ***+ Import a new update***.
4. Select ***+ Select from storage container***.
5. Click on the name of the blob storage which contains the container that stores the manifest files and binary images.
6. Click on the container that stores the manifest files and binary images.
7. Check the boxes for all the files in the list and then click the ***Select*** button at the bottom of the page.

A screenshot of a computer program

Description automatically generated with low confidence

1

1. Confirm that the manifest and binaries show up on the resulting page. Click the ***Import update*** button at the bottom of the page.

A screenshot of a phone

Description automatically generated with medium confidence

CLICK

1. You may get a warning message regarding the status of the import; ignore the message and proceed with the next step.

A screenshot of a message

Description automatically generated with low confidence

1. Confirm that a new update was created showing the correct firmware version number. It may take up to a few minutes for the new update to appear in the list, so click on the ***Refresh*** icon periodically until the WFI32 update shows up in the list (actually now may be a good time for a coffee break).

A screenshot of a computer

Description automatically generated with medium confidence

CLICK

1. Click on the ***Groups and Deployments*** tab.
2. The name of the deployment group that you just created (e.g. “TestDevices”) should show up under the list of device groups. Click on the ***Deploy*** link which should show up under the ***Status*** column for the deployment group.

CLICK

Graphical user interface, text, application, Teams

Description automatically generated

1. The ***New Updates*** pop-up window should appear, showing the correct firmware version for deployment. Click on the 🡪**Deploy** button.

A screenshot of a computer

Description automatically generated with medium confidence

CLICK

1. The ***Create deployment*** pop-up window should appear. Leave the default option as ***Start immediately*** and click on the ***Create*** button to start the deployment.

A screenshot of a application

Description automatically generated with low confidence

1. Go back to observing the terminal output window. You can see the update firmware is pushed from ADU to the device. After completing the upload, the device will reboot with the new firmware.

A screenshot of a computer

Description automatically generated

A screenshot of a computer

Description automatically generated

RESET TRIGGERED

1. To cancel the deployment, click on the **Groups and Deployments** tab and then locate the deployment group (e.g. “TestDevices”) under the list of device groups. Click on the ***Deploy*** link which should show up under the ***Status*** column for the deployment group.

CLICK

Graphical user interface, text, application, Teams

Description automatically generated

1. Locate the name/version of the device update and click on its **View** button.

A screenshot of a computer

Description automatically generated with medium confidence

CLICK

1. On the **Current updates** tab, click on the **Cancel deployment** button.

A screenshot of a computer

Description automatically generated

CLICK

# Clean Up Resources

If you no longer need the Azure resources created in this tutorial, you can use the Azure CLI to delete the resource group and all the resources you created for this tutorial. Optionally, you can use Azure IoT Explorer to delete individual resources including devices and IoT hubs.

If you continue to another tutorial in this getting started guide, you can keep the resources you've already created and reuse them.

Important: Deleting a resource group is irreversible. The resource group and all the resources contained in it are permanently deleted. Make sure that you do not accidentally delete the wrong resource group or resources.

To delete a resource group by name:

1. Run the [az group delete](https://docs.microsoft.com/cli/azure/group?view=azure-cli-latest#az-group-delete) command. This removes the resource group, the IoT Hub, and the device registration you created.

az group delete --name MyResourceGroup

1. Run the [az group list](https://docs.microsoft.com/cli/azure/group?view=azure-cli-latest#az-group-list) command to confirm the resource group is deleted.

az group list

# Next Steps

In this tutorial you created an IoT Hub and added the Device Update resource to it. Then you prepared and deployed the new firmware for the dev board and the simulated leaf device.

To learn more about the APIs of the Device Update agent for Azure RTOS, or the Device Update for IoT Hub service, view <https://aka.ms/azrtos/adu>

To learn more about Azure RTOS and how it works with Azure IoT, view <https://azure.com/rtos>.